# CE 66/ 54 – basket dispenser

**Dimensions**

Length: 885 mm

Width: 700 mm

Height: 911 mm

Height (w/ optional domed lid): 1067 mm

Operating height: 900 mm

**Description**

**Structure**

The basket dispenser is made entirely of CNS 18/10 (AISI 304) with a specially ground matte surface finish (“microlised” surface).

The dispenser has a single-walled body in a closed and compact design that protects the baskets from dirt.

The baskets are placed on a platform. The dispenser’s special construction prevents the baskets from slipping inside the body.

The platform is supported by tension springs. By hanging or unhanging individual springs, the serving height can be adjusted according to the weight of the objects stacked.

A CNS safety push-pull handle with side bumper elements of plastic (polyamide) is mounted at the operator side.

The dispenser is made mobile by corrosion-resistant synthetic castors (4 steering castors, 2 of which have brakes, 125 mm dia.).

Very robust synthetic corner guards (polyamide) at all four corners protect the dispenser from being damaged.

### Accessories / options

* steel wire baskets, plastic-coated

650 x 530 x 75 mm or 650 x 530 x 115 mm

* stainless steel baskets

650 x 530 x 75 mm or 650 x 530 x 115 mm

* domed lid (710 x 590 mm), polycarbonate

stacking height w/ domed lid: 680 mm

stacking height w/o domed lid: 540 mm

* coloured panelling
* for other castor variations, please refer to our general price list

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 48 kg

Platform: 660 x 540 mm

Capacity: 6 baskets, each 115 mm high,

9 baskets, each 75 mm high

Emissions: The workplace-specific noise level of the unit is less than 70 dB(A)

### Special features

* protected against splash and jet water (IPX 5)
* VDE tested, GS certified
* adjustable spring tension
* complies with DIN 18665, Part 6

**Make**

Manufacturer: B.PRO

Model: CE 66/ 54

Order No.: 574 906