# CE 54/ 38 – Tray dispenser

**Dimensions**

Length: 775 mm

Width: 520 mm

Height: 911 mm

Operating height: 900 mm

**Description**

**Structure**

The tray dispenser is made entirely of CNS 18/10 (AISI 304) with a specially ground matte surface finish (“microlised” surface).

It features a single-walled closed construction. The trays are placed on a platform. Its interior panelling is entirely powder-coated to prevent the trays from slipping and getting damaged.

The platform is supported by tension springs. By hanging or unhanging individual springs, the serving height can be adjusted according to the weight of the objects stacked.

A CNS safety push-pull handle with side bumper elements of plastic (polyamide) is mounted at the operator side.

The dispenser is made mobile by corrosion-resistant synthetic castors (4 steering castors, 2 of them with brakes, 125 mm ø). Very robust synthetic corner guards (polyamide) at all four corners protect the trolley from being damaged.

### Accessories / options

* coloured panelling
* cutlery holder with or without napkin dispenser
* for other castor variations, please refer to our general price list

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 37 kg

Capacity: approx. 80 trays,

 530 x 370 mm

Stacking height: 540 mm

Emissions: The workplace-specific noise level of the unit is less than 70 dB(A)

**Special features**

* adjustable spring tension
* complies with DIN 18665, Part 6

**Make**

Manufacturer: B.PRO

Model: CE 54/38

 B.PRO INMOTION

Order no. 574 908