# UNI 59/ 29 – universal dispenser

**Dimensions**

Length: 740 mm

Width: 520 mm

Height: 944 mm

Height (w/ optional domed lid): 1027 mm

Operating height: 900 mm

**Description**

**Structure**

The universal dispenser is made entirely of CNS 18/10 (AISI 304) with a specially ground matte surface finish (“microlised” surface).

It has a single-walled body in a closed and compact design. The interior is lined entirely with a powder-coated panelling to avoid marks on the crockery.

The frame of the platform has been designed so that it allows for stacking a wide variety of different types of crockery with the help of 6 synthetic guide rods that can be variably positioned.

The stacking platform runs smoothly and has ball-bearing roller guides to secure it against tilting and jamming.

The platform is supported by tension springs. By hanging or unhanging individual springs, the serving height can be adjusted according to the weight of the objects stacked.

A CNS safety push-pull handle with side bumper elements of plastic (polyamide) is mounted at the operator side.

The dispenser is made mobile by corrosion-resistant synthetic castors (4 steering castors, 2 of which have brakes, 125 mm dia.).

Very robust synthetic corner guards (polyamide) at all four corners protect the dispenser from being damaged.

### Accessories / options

* domed lid (642 x 342 mm), polycarbonate

stacking height w/ domed lid: 680 mm

stacking height w/o domed lid: 540 mm

* coloured panelling
* for other castor variations, please refer to our general price list

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 48,5 kg

Interior dims.: 590 x 290 mm

Capacity: depends on type of crockery

Emissions: The workplace-specific noise level of the unit is less than 70 dB(A)

### Special features

* protected against splash and jet water (IPX 5)
* adjustable spring tension
* variable setting due to 6 guide rods
* complies with DIN 18665, Part 6

**Make**

Manufacturer: B.PRO

Model: UNI59/ 29

Order No.: 574 911