# CCE 53/ 53 – basket dispenser

**Dimensions**

Length: 810 mm

Width: 555 mm

Height: 900 mm

**Description**

**Structure**

The basket dispenser is made entirely of CNS 18/10 (AISI 304) with a specially ground matte surface finish (“microlised” surface).

It is an open construction. The baskets are placed on a platform with all-round turned up edges that hold them in place.

The platform is supported by tension springs. By hanging or unhanging individual springs, the serving height can be adjusted according to the weight of the objects stacked.

A CNS safety push-pull is mounted at the operator side.

The dispenser is made mobile by corrosion-resistant synthetic castors (4 steering castors, 2 of which have brakes, 125 mm dia.).

Very robust synthetic corner guards (polyamide) at all four corners protect the dispenser from being damaged.

### Accessories / options

* steel wire baskets, plastic-coated

500 x 500 x 75 mm or 500 x 500 x 115 mm

525 x 525 x 75 mm or 525 x 525 x 115 mm

* stainless steel baskets

500 x 500 x 75 mm or 500 x 500 x 115 mm

525 x 525 x 75 mm or 525 x 525 x 115 mm

* cutlery holder with or without napkin dispenser
* for other castor variations, please refer to our general price list

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 33 kg

Interior dims.: 536 x 536 mm

Capacity: 6 baskets, each 115 mm high,

 9 baskets, each 75 mm high

Stacking height: 700 mm

Emissions: The workplace-specific noise level of the unit is less than 70 dB(A)

Max. load: 200 kg

### Special features

* adjustable spring tension
* complies with DIN 18665, Part 6

**Make**

Manufacturer: B.PRO

Model: CCE 53/ 53

Order No.: 574 917