# BTA 3 – Transport and Serving Trolley



##### Dimensions

Length: 1060 mm

Width: 770 mm

Height: 840 mm

Shelf dimensions: 940x700 mm

Spacing between shelves: 300 mm

**Design**

The transport and serving trolley with two support shelves is made completely of CNS 18/10, and the surface is micro-polished.

1 curved push handle of stable square tubing (25x25 mm) is mounted on each short end. To improve the stability, a longitudinal profile is mounted on the lower side of the upper shelf.

The lower shelf can, for example, be used as a support for the B.PROTHERM lid.

The BTA 3 can be moved on stainless synthetic castors pursuant to DIN 18867-8 (4 steering castors, 2 of which have locking brakes with a diameter of 125 mm).

Solid synthetic (polyethylene) corner guards at all four corners protect against damage.

**Technical data**

Material: CNS 18/10, polyetyhlene

Weight: 31 kg

Max. load-bearing capacity: 150 kg

Max. load per shelf. 100 kg

Capacity: 2 x BPT 160 K, or

2 x BPT 320 ECO/K/KB/KBR, or

2 x BPT 420 K/KBUH/KBRUH, or

2 x BPT 620

K/KBUH/KBRUH

**Make**

Manufacturer: B.PRO

Model: BTA 3

Order No.: 574 987