# Platform trolley BTT 10 x 8

**Dimension**

Length: 1035 mm

Width: 770 mm

Height: 840 mm

Platform height: 230 mm

**Description**

The platform trolley is made entirely of CNS 18/10 (AISI 304) with a smooth surface finish (“microlised” surface).

At one of its short sides, the trolley has a curved handle of 25 x 25 mm rectangular tube, which is further stabilised by 2 laterally welded beams. The underside of the platform features reinforcing support bars.

The trolley can be moved on stainless synthetic castors pursuant to DIN 18867, Part 8 (2 fixed castors and 2 steering castors with brakes, castor diameter 125 mm). All four corners are equipped with very robust corner guards.

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 20 kg

Max. load: 250 kg

Platform size: 940 x 700 mm

**Make**

Manufacturer: B.PRO

Model: BTT 10 x 8

Order No.: 574 989