# Platform trolley PFWP 10 x 6

**Dimension**

Length: 1139 mm

Width: 690 mm

Height: 950 mm

Platform height: 252 mm

**Description**

The platform trolley consists of a loading shelf with all-round profiled edge that is folded down on all sides. On its underside, the shelf is equipped with reinforcing sectional bars.

At one of its short sides, the trolley has a curved handle of 25 x 25 mm rectangular tube, which is further stabilised by 2 laterally welded beams.

The underside of the platform features reinforcing support bars.

The trolley can be moved on galvanized steel castors (2 fixed castors and 2 steering castors with brakes, castor diameter 160 mm). The castors are mounted to special reinforcing sectional bars, providing for a much higher load capacity. All four corners are equipped with very robust corner guards.

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 24 kg

Max. load: 400 kg

Platform size: 1020 x 620 mm

### Special features

* All-round profiled edge. Extremely high load capacity of 400 kg.
* Curved handle for easy pushing

**Make**

Manufacturer: B.PRO

Model: PFWP 10 x 6

Order No.: 574 991