# Platform trolley BTT 8 x 6

**Dimension**

Length: 651 mm

Width: 770 mm

Height: 950 mm

Platform height: 230 mm

**Description**

The platform trolley is made entirely of CNS 18/10 (AISI 304) with a smooth surface finish (“microlised” surface).

At the short side, the trolley has a curved handle of 25 x 25 mm rectangular tube.

The trolley can be moved on stainless synthetic castors pursuant to DIN 18867, Part 8 (4 steering castors, 2 of them with brakes, castor diameter 125 mm). All four corners are equipped with very robust corner guards.

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 11 kg

Max. load: 100 kg

Platform size: 500 x 700 mm

Capacity: 4 pcs. BPT 160 K, or

 3 pcs. BPT 320 ECO/K/ KB/KBR, or

 2 pcs. BPT 420 K/ KBUH/ KBRUH, or

 2 pcs. BPT 620 K/KBUH/ KBRUH

### Special features

* Curved handle for easy pushing

**Make**

Manufacturer: B.PRO

Model: BTT 8 x 6

Order No.: 574 992