# Platform trolley PFWP 8 x 5

**Dimension**

Length: 939 mm

Width: 590 mm

Height: 950 mm

Platform height: 237 mm

**Description**

The platform trolley consists of a loading shelf with all-round profiled edge that is folded down on all sides. On its underside, the shelf is equipped with reinforcing sectional bars and a sound absorbing lining. The chassis is made of a robust, continuous round tube frame construction (dia. 25 mm) that at the same time serves as a trolley handle.

The trolley can be moved on galvanized steel castors (2 fixed castors and 2 steering castors with brakes, castor diameter 125 mm). The castors are mounted to cross support rails, providing for a high load capacity. All four corners are equipped with robust corner guards.

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 19 kg

Max. load: 350 kg

Platform size: 820 x 520 mm

### Special features

* All-round profiled edge
* Curved handle for easy pushing

**Make**

Manufacturer: B.PRO

Model: PFWP 8 x 5

Order No.: 575004