# Transport trolley TRE 6 x 4

**Dimension**

Length: 742 mm

Width: 430 mm

Height: 950 mm

Platform height: 201 mm

**Description**

The platform trolley for Euro containers is made entirely of CNS 18/10 (AISI 304) with a smooth surface finish (“microlised” surface).

At the short side, the trolley has a curved handle of 25 x 25 mm rectangular tube

The trolley can be moved on stainless synthetic castors pursuant to DIN 18867, Part 8 (4 steering castors, 2 of them with brakes, castor diameter 125 mm). All four corners are equipped with robust corner guards (Polyethylen).

**Tecnical data**

Material: CNS 18/10

Weight: 10 kg

Max. load: 120 kg

Platform size: 600 x 400 mm

### Special features

* Ergonomic push handle

**Make**

Manufacturer: B.PRO

Model: TRE 6 x 4

Order No.: 575 098