# TWE 6 x 4 transport trolley

**Dimensions**

Length: 940 mm

Width: 700 mm

Height: 1,585 mm

**Design**

The transport trolley for Euro containers is made completely of stainless steel. The surface is micro-polished.

The trolley is made of a 25 x 25 mm welded square tube construction. 2x push-through protection at the rear and one vertical push-through protection on each short side give the transport trolley additional stability.

Two welded-in, closed stainless-steel shelves, one of which functions as the base bottom and the second as a middle shelf with a spacing of 724 mm, offer space for 6 600 x 400 mm Euro containers each.

Two push handles on the body enable simple trolley manoeuvring.

The trolley is mobile on galvanised steel castors   
(2 fixed and 2 steering castors with brakes, castor diameter 160 mm). Solid synthetic (polyamide) corner guards at all four corners protect against damage.

### Options

* 2x push-through protection made of 15 x 15 mm stainless steel at front, can be swivelled

**Technical data**

Material: Stainless steel

Weight: 50 kg

Total load-bearing  
capacity: 350 kg

Capacity: 12 600 x 400 mm   
Euro containers

**Make**

Manufacturer: B.PRO

Model: TRE 6 x 4

Order no. 575 101