# RWR-E 6x4 shelf trolley

**Dimensions**

Length: 686 mm

Width: 536 mm

Height: 1,515 mm

Inside dimensions:

Spacing between support rails: 245 mm

**Design**

The shelf trolley consists of stainless steel,
AISI 304. Welded-in guide rails are located between the sturdy 25 x 25 mm square tube (curved without tapering). These are equipped with push-through protection on both sides for the lengthwise insertion of Euro containers.

A 20 x 10 mm welded-in square tube at mid-height offset on both the front and back of the shelf trolley provides additional stability.

The shelf trolley is mobile on galvanised steel castors (4 steering castors, 2 of which have brakes, castor diameter 125 mm). Synthetic (polyamide) wall guards at all four corners protect against damage.

**Technical data**

Material: Stainless steel Polyamide (PA)

Material thickness
of the square tube: 1.5 mm

Material thickness
of the support rails:

 1.25 mm

Weight: 14 kg

Load-bearing capacity
per trolley: 125 kg

Number of support
pairs: 5

Capacity: 5 E2 Euro containers

### Special features

* Guide rails with push-through protection on both sides

**Make**

Manufacturer: B.PRO

Model: RWR-E 6x4

Order no. 572 103