# RWR-B 6x4-20 shelf trolley

**Dimensions**

Length: 686 mm

Width: 536 mm

Height: 1,729 mm

Inside dimensions:

Spacing between support rails: 73 mm

**Design**

The shelf trolley consists of stainless steel,   
AISI 304. Welded-in guide rails are located between the sturdy 25 x 25 mm square tube (curved without tapering). These are equipped with push-through protection on both sides for the lengthwise insertion of 60x40 cm baking trays.

A 20 x 10 mm welded-in square tube at mid-height offset on both the front and back of the shelf trolley provides additional stability.

The shelf trolley is mobile on corrosion-resistant synthetic castors pursuant to DIN 18867, Part 8   
(4 steering castors, 2 of which have brakes, castor diameter 125 mm). Synthetic (polyamide) wall guards at all four corners protect against damage.

**Technical data**

Material: Stainless steel Polyamide (PA)

Material thickness   
of the square tube: 1.5 mm

Material thickness   
of the support rails:

1.25 mm

Weight: 21.5 kg

Load-bearing capacity  
per trolley: 200 kg

Number of support  
pairs: 20

Capacity: 20 60x40 cm baking trays

### Special features

* Guide rails with push-through protection on both sides

**Make**

Manufacturer: B.PRO

Model: RWR-B 6x4-20

Order no. 575 104