# B.PROTHERM BPT E 2 x 18 duo H/H



**Dimensions**

Length: 1026 mm

Width: 821 mm

Height: 1072 mm

**Model**

**Design**

The B.PROTHERM is made of AISI 304 stainless steel. The surface is micro-polished.

Body and hinged doors are double-walled and fitted with CFC-free PUR foam panels for thermal insulation. As a duo model, the trolley features two separate, thermally insulated compartments side by side.

The left and right compartments are convection-heated and can be heated and adjusted separately from one another.

The B.PROTHERM is mobile thanks to corrosion-resistant synthetic castors as per DIN 18867, Part 8 (2 fixed and 2 steering castors with brakes, castor diameter 125 mm). The sturdy, synthetic base structure with integrated all-round bumper rail protects the unit and furniture from damage.

**Body**

The base and rear and side walls are fitted with all-round edge radius R2 and are spot-welded at their points of contact (hygienic type HS). The interior is fully equipped with 18 pairs of deep-drawn stainless steel ledge walls per compartment for easy cleaning and maximum hygiene. The support ledges have a uniform spacing of 38.3 mm to hold Gastronorm containers size GN 1/1 or their subdivisions. This means all common spacing dimensions (about 75 mm, 115 mm) can be housed in a single unit and ensures efficient use of the interior.

A heating module with convection heating is permanently fitted into the rear panel of each compartment. Control range: +30 °C to +95 °C. The temperature can be regulated down to the degree in each compartment.

There is an air baffle in front of the heating module on the rear panel in the interior body. This ensures optimum, rapid, uniform air circulation throughout the interior and also serves as a stop for inserted GN containers. The air baffle can be removed for cleaning purposes.

Interior and exterior body are vertically connected with synthetic profiles and thermally separated.

The B.PROTHERM is fitted with 2 horizontal push handles on the left and right short sides as standard. The ergonomic positioning of the handles makes the trolley easy to manoeuvre.

The push handles are inside the bumper rail. The helix cord and plug holder are attached on the unit rear and also within the all-round bumper rail.

A B.PRO controller is integrated into the top of the unit above each compartment, ensuring user-friendly operation. It contains the unit on/off button, a menu button, a function button and an up/down button to precisely regulate the temperature in the interior concerned among other things.

**Doors**

The trolley is equipped with two doors on its front that can be opened 270° and features a lock on its bottom plate. The doors are inside the bumper rail when open or closed and are thus protected from damage. The push handles are still accessible when the door is open. The robust door hinges are made of stainless steel investment casting. The hinge design eliminates risk of injury if a user should accidentally take hold of the hinge. A ventilation flap is fitted into the doors to the compartments to regulate moisture in the container interior.

The doors are also fitted with an all-round, food-safe seal (TPE) that closes against the trolley body and can be removed.

The doors are fitted with a 2-point locking system. It is easy to open from the outside by simply pushing up the door handle.

The B.PROTHERM has a push-button which glows in the dark in its interior. The patented panic opening can be identified if someone should get accidentally locked inside the interior and the door lock can be unlocked from the inside by pressing the button. What is known as the afterglow effect meets the requirements for safety-relevant components specified in ISO 16069.

**Options**

* Can be customised with powder coating on body and doors in 12 colours
* Digitisation/connectivity for digital hygiene, temperature and process management using optionally built-in sensor technology
* Additional socket on rear panel (instead of plug holder) for coupling additional units
* Top with stainless steel railing on 3 sides
* Top with stainless steel railing on 4 sides
* Draw bar and coupling made of stainless steel (please ensure that drawbar and coupling of trolley and towing machine match).
	+ Transfer height 110-200 mm (for rollers ø160 mm)
	+ Transfer height 150-240 mm (for rollers ø200 mm)
	+ Diameter of coupling pin: 25 mm
	+ Diameter drawbar mount: 27 mm
* Hygienic type H1
* Door, lockable
* Convenient door opening with foot operation
* Stainless-steel castors, 125 mm in diameter, 2 fixed and 2 steering castors with brakes
* Anti-static castors, 125 mm in diameter, 2 fixed and 2 steering castors with brakes, corrosion-resistant in compliance with DIN 18867-8, synthetic
* Galvanised steel castors, 160 mm in diameter, 2 fixed and 2 steering castors with brakes
* Galvanised steel castors with elastic tyres, 160 mm in diameter, 2 fixed and 2 steering castors with brakes
* Stainless-steel castors, 160 mm in diameter, 2 fixed and 2 steering castors with brakes
* Stainless-steel castors with elastic tyres, 160 mm in diameter, 2 fixed and 2 steering castors with brake

**Accessories**

* Eutectic plate -3 °C, synthetic

(Order no.: 568 136)

* Eutectic plate -12 °C, synthetic

(Order no.: 573 332)

* Slide-in frame to sub-divide GN containers

with max. depth 150 mm (order no. 564 352)

* GN support bars for variable insertion of GN containers of the size GN 1/4, GN 1/6, GN 1/9 in the slide-in frame (ST 3 order no. 550 650; ST 5 order no. 550 651)
* Menu card holder for the door on front, stainless steel, to attach DIN A5 and DIN A6 menu cards (order no. 575 230)
* BPT E menu card, DIN A6 (order no. 564 353)
* Special pen for marking BPT E menu cards (order no. 564 361)
* Menu card box, synthetic (order no. 564 355)

**Technical data**

Material: Stainless steel,

 synthetic

Insulating material: PUR foam panels, CFC-free

Weight: 110 kg

Capacity: 9 x GN 1/1-65 per compartment

 2 x 18 pairs of deep-drawn support ledges

 Space between ledges of 38.3 mm

Protection type: IPX5

Connected load: 220–240 V AC/50–60 Hz/

 0.8 kW

temperature range: +30 °C to +95 °C\*

Emissions: The workplace-specific noise level for the unit is less than 70 dB(A)

\* Measured at the container's geometrical centre

**Special features**

* The compartments can be heated and adjusted separately from one another
* Extremely efficient, flexible use of interior thanks to uniform space between ledges of 38.3 mm
* Deep-drawn stainless steel ledge walls for easy cleaning and maximum hygiene.
* Sturdy, enclosed, solid, synthetic base structure with integrated all-round bumper rail.
* Hinged door with door opening of 270°, with lock
* Optional connectivity function

**Make**

Manufacturer: B.PRO

Model: BPT E 2 x 18 duo H/H

 B.PROTHERM

Order no. 575 206