# CE 65/45 platform dispenser

**Dimensions**

Length: 893 mm

Width: 578 mm

Height: 911 mm

**Model**

**Design**

The dispenser housing is made of high-quality, corrosion-resistant stainless steel. The surface is micro-polished.

The platform is used to hold various types of dishes. Depending on stacked items, a range of platforms are available.

The platform dispenser has continuous, powder-coated inner panelling to stop dishes from sliding, thus preventing damage to the body interior.

To ensure a consistently even serving height, the spring tension can be regulated depending on the stacked items by hooking or unhooking the tension springs.

A stainless-steel safety push handle with synthetic (polyamide) side corner guard elements is attached to the operator side.

The dispenser can be moved on its corrosion-resistant synthetic castors (4 steering castors, 2 of which have brakes, 125 mm in diameter). Solid synthetic (polyamide) corner guards at all four corners protect against damage.

### Accessories/options

* Push handles as tube clamp made completely of stainless steel
* All-round impact bars made of PE
* All-round impact bars, reinforced (milled)
* Galvanised steel castors, 4 steering castors, 2 of which have brakes, 125 mm dia.
* Stainless-steel castors, 4 steering castors,
2 of which have brakes, 125 mm dia.

**Technical data**

Material: Stainless steel

Weight: approx. 60 kg

Max. load: 220 kg

Capacity: dependent on type of dishes

Loading:

(Platform for:) Soup bowls 0.35 l, 104 mm dia., approx. 600 pcs.

 Side bowls 122 x 89 mm
 approx. 950 pcs.

Serving height: 900 mm

Inside dimensions: approx. 656 x 456 mm

Stacking height: approx. 600 mm

### Special features

* Spring tension can be changed
* As per DIN 18665, Part 9

**Make**

Manufacturer: B.PRO

Model: CE 65/45

Order No.: 575289