# CEK 65/45 platform dispenser with cooling slits

**Dimensions**

Length: 893 mm

Width: 579 mm

Height: 911 mm

**Model**

**Design**

The dispenser housing is made of high-quality, corrosion-resistant stainless steel. The surface is micro-polished. The body features cooling slits to ensure the even temperature distribution of dishes during cooling in the cold storage rooms.

The platform is used to hold various types of dishes. Depending on stacked items, a range of platforms are available.

The platform dispenser has continuous, powder-coated inner panelling to stop dishes from sliding, thus preventing damage to the body interior.

To ensure a consistently even serving height, the spring tension can be regulated depending on the stacked items by hooking or unhooking the tension springs.

A stainless-steel safety push handle with synthetic (polyamide) side corner guard elements is attached to the operator side.

Thanks to its stainless-steel synthetic castors (4 steering castors, 2 of which have brakes, 125 mm dia.), the dispenser is fully mobile. Solid synthetic (polyamide) corner guards at all four corners protect against damage.

### Accessories/options

* Push handles as tube clamp made completely of stainless steel
* All-round impact bars made of PE
* All-round impact bars, reinforced (milled)
* Galvanised steel castors, 4 steering castors, 2 of which have brakes, 125 mm dia.
* Stainless-steel castors, 4 steering castors,
2 of which have brakes, 125 mm dia.

**Technical data**

Material: Stainless steel

Weight: approx. 58 kg

Max. load: 220 kg

Capacity: dependent on type of dishes

Loading:

(Platform for:) Soup bowls 0.35 l,
104 mm dia., approx. 600 pcs.

 Side bowls 122 x 89 mm
 approx. 950 pcs.

Serving height: 900 mm

Inside dimensions: approx. 656 x 456 mm

Stacking height: approx. 600 mm

### Special features

* Spring tension can be changed
* Body with cooling slits
* As per DIN 18665, Part 9

**Make**

Manufacturer: B.PRO

Model: CEK 65/45

Order no.: 575290