**B.PRO selectively controlled mixer tap**

**230 V**

**Design:**

Contactless, electronically controlled single-hole mixer tap.

* Sensor in the mixer tap
* Contactless activation through infrared electronics
* Temperature can be adjusted via side lever
* Chrome-plated
* 24 hours hygiene flushing
* Mains adapter

**Technical data:**

* Mains operation 220–204 V 50/60 Hz 1/N/PE 6 W
* Operating pressure 0.5–10 bar
* Flow rate max. 6 l/min (3 bar)
* Protection type IP 65 (the mixer tap is protected against dust and spray water (nozzle) in accordance with DIN EN 60529.)
* Water temperature max. 80 °C (10 min.)
* Suggested water temperature 5 - 60 °C
* Water run-on time (default setting) 1 second
* Water flow time"24 hours hygiene flushing":30 seconds
* Corner valve connection: standard G 3/8´´

**Make:**

Manufacturer: B.PRO

Model: selectively controlled mixer tap 230 V

Order no.: 575330