**B.PRO selectively controlled mixer tap**

**with battery**

**Design:**

Contactless, electronically controlled single-hole mixer tap.

* Sensor in the mixer tap
* Contactless activation through infrared electronics
* Temperature can be adjusted via side lever
* Chrome-plated
* 24 hours hygiene flushing
* With external battery compartment

**Technical data:**

* Battery operation: 4x AA batteries

each with 1.5 V

* Operating pressure: 0.5–10 bar
* Flow rate: max. 6 l/min (3 bar)
* Protection type: IP 65 (the mixer tap is protected against dust and spray water (nozzle) in accordance with DIN EN 60529.)
* Water temperature: max. 80 °C (10 min.)
* Suggested water temperature: 5 - 60 °C
* Water run-on time (default setting): 1 second
* Water flow time"24 hours hygiene flushing":

30 seconds

* Corner valve connection: standard G 3/8´´

**Make:**

Manufacturer: B.PRO

Model: selectively controlled mixer tap with battery

Order no.: 575331