**BCTT 3 beverage crate transport trolley**

**Dimensions**

Length: 468 mm

Width: 673 mm

Height: 1550 mm

Height incl. trolley top (optional): 1586 mm

**Model**

The beverage crate transport trolley is a one-piece model made completely of stainless steel, AISI 304. The frame construction is made of sturdy square tube (25x25 mm and 40x20 mm) and is welded all round.

The stainless-steel supports are welded to the frame construction and slope towards the rear. Bevels on the sides and back of the supports ensure a firm hold for beverage crates.

The beverage crate transport trolley has a capacity of three beverage crates (max. 400 x 330 x 350 mm).

The trolley is mobile on corrosion-resistant synthetic castors pursuant to DIN 18867, Part 8 (4 steering castors, 2 of which have brakes, castor diameter 125 mm). Synthetic (polyamide) round wall guards at all four corners protect against damage.

**Accessories/options**

* Thin sheet panelling on 2 sides, electrolytically galvanised on both sides, powder-coated in various colours, for mounting on the beverage crate transport trolley. Can be easily removed without any tools for cleaning.
* Stainless-steel panelling on 2 sides, for mounting on the beverage crate transport trolley. Can be easily removed without any tools for cleaning.
* Thin sheet panelling on 3 sides, electrolytically galvanised on both sides, powder-coated in various colours, for mounting on the tray clearing trolley. Can be easily removed without any tools for cleaning.
* Stainless-steel panelling on 3 sides, for mounting on the tray clearing trolley. Can be easily removed without any tools for cleaning.
* Stainless-steel trolley top with all-round railing. For mounting on the beverage crate transport trolley. Can be easily removed without any tools for cleaning. The maximum surface load is 20 kg.

**Technical data**

Material: Stainless steel, polyamide (PA)

Weight: Approx. 21 kg

Max. load-bearing
capacity trolley: 70 kg

Capacity: 3 beverage crates (max. 400 x 330 x 350 mm)

### Special features

* Sturdy stainless-steel frame construction
* Welded supports for beverage crates, sloped with raised edge for a secure hold
* Optional panelling for mounting on the BCTT. Can therefore be easily removed for cleaning
* Attachments like panelling and top can be retrofitted at any time.

**Make**

Manufacturer: B.PRO

Model: BCTT 3

Order no.: 575384