# CEB 50/ 50 – basket dispenser

**Dimensions**

Length: 600 mm

Width: 545 mm

Height: 765 to 865 mm

**Description**

**Structure**

The build-in basket dispenser is made entirely of CNS 18/10 (AISI 304) with a specially ground matte surface finish (“microlised” surface).

It is an open model designed for being built in from below.

The baskets are placed on a platform with all-round turned up edges that hold them in place.

The platform is supported by tension springs. By hanging or unhanging individual springs, the serving height can be adjusted according to the weight of the objects stacked.

### Accessories / options

* steel wire baskets, plastic-coated

500 x 500 x 75 mm or 500 x 500 x 115 mm

* stainless steel baskets

500 x 500 x 75 mm or 500 x 500 x 115 mm

* domed lid (557 x 557 mm), polycarbonate

stacking height w/ domed lid: 540 mm

stacking height w/o domed lid: 680 mm

* installation from below, with all-round flange

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 19 kg

Interior dims.: 520 x 520 mm

Capacity: 6 baskets, each 115 mm high,

9 baskets, each 75 mm high

Emissions: The workplace-specific noise level of the unit is less than 70 dB(A)

### Special features

* protected against splash and jet water (IPX 5)
* adjustable spring tension
* complies with DIN 18665, Part 6

**Make**

Manufacturer: B.PRO

Model: CEB 50/ 50

B.PRO INMOTION

Order No.: 590 025