# Soap and disinfectant dispenser TV 25

**Dimensions**

Width: 94 mm

Height: 273 mm

Depth: 162 mm

**Design**

The soap and disinfectant dispenser features a polished stainless-steel housing and a synthetic wall mount. Suitable for 1000 ml bottles, the dispenser is fitted with a lockable cover panel and a short operating lever
(with about 80 mm of lever visible). The 25 mm stainless-steel pump with a straight suction hose can be autoclaved and can dose about 0.7, 1.0 or 1.5 ml of liquid soap, alcohol-based disinfectant, lotions or similar.

**Technical data**

Material: Polished stainless steel housing; synthetic wall mount

Fill level: 1000 ml

### Special features

* Replaceable pump; dispenser and pump can be sterilised in an autoclave at 134 °C for 20 min. at
2 bar.

**Make**

Manufacturer: B.PRO

Model: TV 25

Order no. 144665