**Built-in basin EE 5x5-4.3**

**Dimensions:**

Exterior dimensions:

Length: 500 mm

Width: 500 mm

Basin size:

Length: 400 mm

Width: 400 mm

Depth: 300 mm

Cut-out dimensions:

Length: 480 mm

Width: 480 mm

**Design:**

Basin and top surface deep-drawn. With securing elements and suitable all-around seal; for building into Resopal or AISI 304 table tops.

Basin surface fully brushed; basin without overflow indentation.

Drain: 1 ½".

**Accessories:**

* 1 ½" tube overflow Order No.: 223 063

**Technical data:**

Material: Stainless steel

Material no.: 1.4301

**Make:**

Manufacturer: B.PRO

Model: EE 5x5-4,3

Order No.: 504 032