**Built-in glass-rinsing basin EE 3.8x5.8**

**Dimensions:**

Exterior dimensions:

Length: 380 mm

Width: 580 mm

Basin size:

Length: 302 mm

Width: 502 mm

Depth: 300 mm

Cut-out dimensions:

Length: 360 mm

Width: 560 mm

**Design:**

Basin and top surface deep-drawn. With securing elements and suitable all-around seal; for building into Resopal or AISI 304 table tops.

Basin surface fully brushed; basin without overflow indentation.

Drain: 1 ½".

**Accessories:**

* 1 ½" tube overflow: Order No.: 223 063

**Technical data:**

Material: Stainless steel

Material no.: 1.4301

**Make:**

Manufacturer: B.PRO

Model: EE 3,8x5,8

Order No.: 505 035