**Hand-washing basin**

**Dimensions:**

Length: 550 mm

Width: 450 mm

Height: 180 mm

Basin size:

Length: 500 mm

Width: 300 mm

Depth: 150 mm

**Design:**

The top surface turned down on all sides. 1 deep-drawn washbasin seamlessly welded into surface. 1 1/2" drain, with overflow protection, without valve. 2 stainless-steel brackets welded on. With stainless steel basin panelling on three sides, 150 mm high.

**Technical data:**

Material: Stainless steel

DIN 1.4301

**Special options:**  See GWS-OPT.

**Make:**

Manufacturer: B.PRO

Model: WB 5.5 x 4.5 x 1.5

Order No.: 507 009

**Accessories: Order No.:**

1 1/2" overflow valve 223 063