**Built-in basin EE 4x4**

**Dimensions:**

Exterior dimensions:

Length: 435 mm

Width: 470 mm

Basin size:

Length: 340 mm

Width: 370 mm

Depth: 150 mm

Cut-out dimensions:

Length: 415 mm

Width: 450 mm

**Design:**

Basin and top surface deep-drawn. With securing elements and suitable all-around seal; for building into Resopal or AISI 304 table tops.

Basin surface: Natural finish, basin without overflow indentation.

Drain: 1 ½".

**Accessories:**

* 1 ½" tube overflow Order No.: 223 063

**Technical data:**

Material: Stainless steel (AISI 304)

Material no.: 1.4301

**Make:**

Manufacturer: B.PRO

Model: EE 4x4

Order No.: 531 282