# Storage and garbage container VBR 400K

**Dimension**

Diameter: 430 mm

Height: 495 mm

**Description**

The container of CNS 18/10 (AISI 304) has neither seams nor joints where dirt could settle. It is equipped with stable carrying handles on both sides.

The lid (Diameter: 430 mm, weight: 2 kg) has a folded-down edge that projects over the container and is provided with a deep-drawn recessed handle in its centre. Thanks to a hanging device on the lid's underside, the lid can be hung up either at the outside container rim or vertically at one of the container handles.

The separate chassis (Diameter: 430 mm, height: 100 mm, weight: 2 kg) is made of CNS 18/10 (AISI 304) and can be moved on galvanized steel castors (4 steering castors, diameter 75 mm).

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 12, 5 kg

Capacity: 50 l

**Make**

Manufacturer: B.PRO

Model: VBR 400 K

Order No.: 565913