# All-purpose trolley AZWA 8 x 5

**Dimension**

Length: 865 mm

Width: 565 mm

Height: 800 mm

**Description**

The multipurpose trolley consists of a CNS 18/10 (AISI 304) 20 x 20 mm rectangular tube frame construction.

It has two shelves with all-round profiled edges.

The trolley has 4 corrosion-protected antistatic steering castors of 75 mm in diameter. At all four corners, round wall bumpers are mounted.

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 10 kg

Max. load per shelf: 40 kg

Max. total trolley load: 80 kg

Interior dia. between

shelves: 450 mm

Shelf: 805 x 505 mm

**Make**

Manufacturer: B.PRO

Model: AZWA 8 x 5

Order No.: 569613