# Spice trolley, open model GW 8 x 5-2

**Dimensions**

Length: 900 mm

Width: 600 mm

Height: 950 mm

**Description**

The spice trolley of CNS 18/10 (AISI 304) is made of stable 25 mm round tube. Between the two short sides, there are 2 deep-drawn welded-in 800 x 500 mm shelves with all-round raised profiled edges. The trolley has handles on both short sides. The top shelf is equipped with 2 brackets of round bar steel, which can be used for inserting 8 spice containers GWB 1/6-150 or Gastronorm containers of size 4 x 1/3 or their subdivisions with 1/6 and 1/9 and a max. depth of 150 mm. The lower shelf features a spice jar holder with holes for 8 spice jars.

The trolley can be moved on stainless synthetic castors pursuant to DIN 18867, Part 8 (4 steering castors, 2 of them with brakes, castor diameter 125 mm). Very robust round wall bumpers (polyamide) at all four trolley corners protect the trolley from being damaged.

**Accessories and options**

* Spice container GWB 1/6-150 of CNS 18/10 with folding Plexiglas lid (Order No. 550501)
* Spice jar of synthetic, round, 100 mm dia., 180 mm high, with hinged spout (Order No. 145423)

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 21 kg

Capacity: 8 spice jars; 8 spice containers GWB 1/6-150 or 4 x GN 1/3 or subdivided with GN 1/6

 and GN 1/9, max. depth 150 mm

### Special features

* Railings of stable round bar steel, bolted

**Make**

Manufacturer: B.PRO

Model: GW 8 x 5-2

Order No.: 569790