# Spice trolley, closed model GWL 8 x 6

**Dimensions**

Length: 865 mm

Width: 675 mm

Height: 985 mm

**Description**

The spice trolley of CNS 18/10 (AISI 304) consists of a stable frame construction of 25 x 25 x 1.25 mm rectangular tube. At the left hand top of the trolley, in a frame, 3 spice containers of size GN 1/6-150 with hinged transparent plastic lids are suspended. Next to the spice containers, there are 4 hung-in spice jars with hinged spout. The underframe features 3 tilt-out compartments, each containing a removable synthetic container. Below, 2 big spice drawers and 2 small spice drawers with full telescopic extensions are mounted, each including chrome nickel steel Gastronorm containers (3 x GN 1/3-150, as well as 3 x GN 1/3-100). At the back side of the trolley, 2 galleries are mounted one on top of the other which can hold a total of up to 8 spice bottles.

At one short side, the trolley is equipped with a curved handle of rectangular tube.

The trolley can be moved on stainless synthetic castors pursuant to DIN 18867, Part 8 (4 steering castors, 2 of them with brakes, castor diameter 125 mm). Very robust round wall bumpers (polyamide) at all four trolley corners protect the trolley from being damaged.

**Accessories and options**

* Spice container GWB 1/6-150 of CNS 18/10 with folding Plexiglas lid (Order No. 550501)
* Spice jar of synthetic, round, 100 mm dia., 180 mm high, with hinged spout (Order No. 145423)

**Technical data**

Material: CNS 18/10 (AISI 304)

Weight: 54 kg

Capacity: 3 spice containers GWB 1/6-150, 4 spice jars, 3 tilt drawer surfaces incl. synthetic containers, 3 chrome nickel steel Gastronorm containers GN 1/3-150, as well as 3 GN 1/3-100

### Special features

* The spice trolley is completely equipped

**Make**

Manufacturer: B.PRO

Model: GWL 8 x 6

Order No.: 572358